
[stream setting]
name = "DIVX MPEG4, IPB"				// configuration name
desc = "IBBPBBP..., enable header, search range 128"	// configuration description
compress_mode = 4		// 'MultiMedia.h': EVideoFormat
mpeg4_mode = 1			// WIS: 0, DIVX: 1, MS: 2
sequence = 3			// 'MultiMedia.h': ESequenceMode
gop_mode = 1			// 0: open GOP, 1: closed GOP
gop_size = 90			// maximum count of pictures in a group of picture
search_range = 128		// motion search range, should be 16,32,64 or 128
gop_head_enable = 1		// 0: disable, 1: enable
seq_head_enable = 1		// 0: disable, 1: enable
aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 0		// 0: disable, 1: enable

[stream setting]
name = "DIVX MPEG4, IP Only"				// configuration name
desc = "IPP..., enable header, search range 128"	// configuration description
compress_mode = 4		// 'MultiMedia.h': EVideoFormat
mpeg4_mode = 1			// WIS: 0, DIVX: 1, MS: 2
sequence = 2			// 'MultiMedia.h': ESequenceMode
gop_mode = 1			// 0: open GOP, 1: closed GOP
gop_size = 30			// maximum count of pictures in a group of picture
search_range = 128		// motion search range, should be 16,32,64 or 128
gop_head_enable = 1		// 0: disable, 1: enable
seq_head_enable = 1		// 0: disable, 1: enable
aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 0		// 0: disable, 1: enable

[stream setting]
name = "Microsoft MPEG4, IP Only"	// configuration name
desc = ""				// configuration description
compress_mode = 4		// 'MultiMedia.h': EVideoFormat
mpeg4_mode = 2			// WIS: 0, DIVX: 1, MS: 2
sequence = 2			// 'MultiMedia.h': ESequenceMode
gop_mode = 0			// 0: open GOP, 1: closed GOP
gop_size = 30			// maximum count of pictures in a group of picture
search_range = 64		// motion search range, should be 16,32,64 or 128
gop_head_enable = 0		// 0: disable, 1: enable
seq_head_enable = 0		// 0: disable, 1: enable
aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 0		// 0: disable, 1: enable

[stream setting]
name = "MPEG2, IPB, DVD"	// configuration name
desc = ""			// configuration description
compress_mode = 1		// 'MultiMedia.h': EVideoFormat
sequence = 3			// 'MultiMedia.h': ESequenceMode
gop_mode = 0			// 0: open GOP, 1: closed GOP
gop_size = 15			// maximum count of pictures in a group of picture
search_range = 128		// motion search range, should be 16,32,64 or 128
gop_head_enable = 1		// 0: disable, 1: enable
seq_head_enable = 1		// 0: disable, 1: enable
aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 1		// 0: disable, 1: enable

[stream setting]
name = "MPEG2, IPB"		// configuration name
desc = ""			// configuration description
compress_mode = 1		// 'MultiMedia.h': EVideoFormat
sequence = 3			// 'MultiMedia.h': ESequenceMode
gop_mode = 0			// 0: open GOP, 1: closed GOP
gop_size = 15			// maximum count of pictures in a group of picture
search_range = 128		// motion search range, should be 16,32,64 or 128
gop_head_enable = 1		// 0: disable, 1: enable
seq_head_enable = 1		// 0: disable, 1: enable
aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 0		// 0: disable, 1: enable

[stream setting]
name = "MPEG2, IPONLY"		// configuration name
desc = ""			// configuration description
compress_mode = 1		// 'MultiMedia.h': EVideoFormat
sequence = 2			// 'MultiMedia.h': ESequenceMode
gop_mode = 0			// 0: open GOP, 1: closed GOP
gop_size = 15			// maximum count of pictures in a group of picture
search_range = 128		// motion search range, should be 16,32,64 or 128
gop_head_enable = 1		// 0: disable, 1: enable
seq_head_enable = 1		// 0: disable, 1: enable
aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 0		// 0: disable, 1: enable

[stream setting]
name = "MPEG1, IPB, VCD"	// configuration name
desc = ""			// configuration description
compress_mode = 0		// 'MultiMedia.h': EVideoFormat
sequence = 3			// 'MultiMedia.h': ESequenceMode
gop_mode = 0			// 0: open GOP, 1: closed GOP
gop_size = 15			// maximum count of pictures in a group of picture
search_range = 128		// motion search range, should be 16,32,64 or 128
gop_head_enable = 1		// 0: disable, 1: enable
seq_head_enable = 1		// 0: disable, 1: enable
aspect_ratio = 2		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 1		// 0: disable, 1: enable

[stream setting]
name = "MPEG1, IPB"		// configuration name
desc = ""			// configuration description
compress_mode = 0		// 'MultiMedia.h': EVideoFormat
sequence = 3			// 'MultiMedia.h': ESequenceMode
gop_mode = 0			// 0: open GOP, 1: closed GOP
gop_size = 15			// maximum count of pictures in a group of picture
search_range = 128		// motion search range, should be 16,32,64 or 128
gop_head_enable = 1		// 0: disable, 1: enable
seq_head_enable = 1		// 0: disable, 1: enable
aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
DVD_compliant = 0		// 0: disable, 1: enable

//[stream setting]
//name = "Example Stream Setting"
//desc = "Example Stream Setting"
//compress_mode = 0		// 'MultiMedia.h': EVideoFormat. 0: MPEG1, 1: MPEG2, 3: H.263, 4: MPEG4, 8: MJPEG
//sequence = 3			// 'MultiMedia.h': ESequenceMode. 1: I Only, 2: IP Only, 3: IPB
//gop_mode = 0			// 0: open GOP, 1: closed GOP
//gop_size = 15			// maximum count of pictures in a group of picture
//deinterlace_mode = 1		// 0: use one field, 1: deinterlace, 2: interlace coding
//search_range = 128		// motion search range. Typical value: 16,32,64 or 128. MSFT=64; H.263=32
//gop_head_enable = 1		// 0: disable, 1: enable. MSFT=0; others=1
//seq_head_enable = 1		// 0: disable, 1: enable. MSFT=0; others=1
//aspect_ratio = 1		// 1= 1:1, 2= 4:3, 3= 16:9
//DVD_compliant = 1		// 0: disable, 1: enable

[framerate setting]
name = "NTSC 29.97fps"
desc = "NTSC 29.97fps"
tv_standard =  NTSC		// NTSC or PAL
frame_rate = 30000		// fps * 1001

//[framerate setting]
//name = "NTSC 24fps IVTC"
//desc = "NTSC 24fps IVTC"
//tv_standard =  NTSC		// NTSC or PAL
//frame_rate = 24000		// fps * 1001

[framerate setting]
name = "PAL 25fps"
desc = "PAL 25fps"
tv_standard = PAL		// NTSC or PAL
frame_rate = 25025		// fps * 1001

[framerate setting]
name = "Sensor 29.97fps"
desc = "Sensor 29.97fps"
tv_standard = None		// NTSC or PAL
frame_rate = 30000		// fps * 1001

//[framerate setting]
//name = "Example Framerate Setting"
//desc = "Example Framerate Setting"
//tv_standard = None		// NTSC, PAL or None
//frame_rate = 30000		// fps * 1001

[resolution setting]
name = "NTSC SD"		// configuration name
desc = "NTSC SD"		// configuration description
tv_standard = NTSC		// NTSC or PAL or None
width = 720			// output stream resolution: horizontal size
height = 480			// output stream resolution: vertical size

[resolution setting]
name = "PAL SD"			// configuration name
desc = "PAL SD"			// configuration description
tv_standard = PAL		// NTSC or PAL or None
width = 720			// output stream resolution: horizontal size
height = 576			// output stream resolution: vertical size

[resolution setting]
name = "NTSC SIF"		// configuration name
desc = "NTSC SIF"		// configuration description
tv_standard = NTSC		// NTSC or PAL or None
width = 352			// output stream resolution: horizontal size
height = 240			// output stream resolution: vertical size

[resolution setting]
name = "NTSC VGA"		// configuration name
desc = "NTSC VGA"		// configuration description
tv_standard = NTSC		// NTSC or PAL or None
width = 640			// output stream resolution: horizontal size
height = 480			// output stream resolution: vertical size

[resolution setting]
name = "NTSC QVGA"		// configuration name
desc = "NTSC QVGA"		// configuration description
tv_standard = NTSC		// NTSC or PAL or None
width = 320			// output stream resolution: horizontal size
height = 240			// output stream resolution: vertical size

[resolution setting]
name = "PAL CIF"		// configuration name
desc = "PAL CIF"		// configuration description
tv_standard = PAL		// NTSC or PAL or None
width = 352			// output stream resolution: horizontal size
height = 288			// output stream resolution: vertical size

[resolution setting]
name = "VGA"			// configuration name
desc = "VGA"			// configuration description
tv_standard = None		// NTSC or PAL or None
width = 640			// output stream resolution: horizontal size
height = 480			// output stream resolution: vertical size

[resolution setting]
name = "QVGA"			// configuration name
desc = "QVGA"			// configuration description
tv_standard = None		// NTSC or PAL or None
width = 320			// output stream resolution: horizontal size
height = 240			// output stream resolution: vertical size

//[resolution setting]
//name = "Example Resolution Setting"
//desc = "Example Resolution Setting"
//tv_standard = NTSC		// NTSC, PAL or None
//width = 352			// output stream resolution: horizontal size
//height = 288			// output stream resolution: vertical size
//h_sub_window = 1		// Perform horizontal sub-window. 0: Disable; 1: Enable
//v_sub_window = 1		// Perform Vertical sub-window. 0: Disable; 1: Enable
//h_sub_offset = 100		// Horizontal starting point to perform subwindow. Valid if h_sub_window = 1.
//v_sub_offset = 100		// Vertical starting point to perform subwindow. Valid if v_sub_window = 1.
//h_scale_enb = 0		// Perform horizontal 1/2 scaling. 0: Disable; 1: Enable
//v_scale_enb = 0		// Perform vertical 1/2 scaling. 0: Disable; 1: Enable
//sub_sample = 0		// Perform sub sampling. 0: Disable; 1: Enable       

[bitrate setting]
name = "Constant 6M"		// configuration name
desc = "Constant 6M"		// configuration description
target_bitrate = 6000000	// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 60000000
peak_bitrate = 60000000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 4M"		// configuration name
desc = "Constant 4M"		// configuration description
target_bitrate = 4000000	// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 40000000
peak_bitrate = 40000000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 2M"		// configuration name
desc = "Constant 2M"		// configuration description
target_bitrate = 2000000	// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 20000000
peak_bitrate = 20000000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 1.5M"		// configuration name
desc = "Constant 1.5M"		// configuration description
target_bitrate = 1500000	// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 15000000
peak_bitrate = 15000000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 1M"		// configuration name
desc = "Constant 1M"		// configuration description
target_bitrate = 1000000	// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 10000000
peak_bitrate = 10000000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 750K"		// configuration name
desc = "Constant 750K"		// configuration description
target_bitrate = 750000		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 7500000
peak_bitrate = 7500000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 500K"		// configuration name
desc = "Constant 500K"		// configuration description
target_bitrate = 500000		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 5000000
peak_bitrate = 5000000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 384K"		// configuration name
desc = "Constant 384K"		// configuration description
target_bitrate = 384000		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 3840000
peak_bitrate = 3840000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 256K"		// configuration name
desc = "Constant 256K"		// configuration description
target_bitrate = 256000		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 2560000
peak_bitrate = 2560000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 128K"		// configuration name
desc = "Constant 128K"		// configuration description
target_bitrate = 128000		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 1280000
peak_bitrate = 1280000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 56K"		// configuration name
desc = "Constant 56K"		// configuration description
target_bitrate = 56000		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 560000
peak_bitrate = 560000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "Constant 28K"		// configuration name
desc = "Constant 28K"		// configuration description
target_bitrate = 28000		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
vbv_buffer = 280000
peak_bitrate = 280000
converge_speed = 50
QMin = 2
QMax = 31
WindowSize = 60
Q = 64				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75

[bitrate setting]
name = "High Quality"		// configuration name
desc = "High Quality"		// configuration description
target_bitrate = 0		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
Q = 0				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75
IQ = 2
BQ = 2
PQ = 2

[bitrate setting]
name = "Good Quality"		// configuration name
desc = "Good Quality"		// configuration description
target_bitrate = 0		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
Q = 0				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75
IQ = 8
BQ = 8
PQ = 8

[bitrate setting]
name = "Low Bitrate"		// configuration name
desc = "Low Bitrate"		// configuration description
target_bitrate = 0		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
Q = 0				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75
IQ = 31
BQ = 31
PQ = 31

[bitrate setting]
name = "constant Q"		// configuration name
desc = "constant Q"		// configuration description
target_bitrate = 0		// target bitrate (bps), a non-zero value enables WIS adaptive bitrate control, 0 means no bit rate control
Q = 0				// initial quantizer, will devided by 4, for exmaple, 7 represents 1.75
IQ = 16
BQ = 16
PQ = 16

//[bitrate setting]
//name = "Example Bitrate Setting"
//desc = "Example Bitrate Setting"
//target_bitrate = 4000000	// Target bitrate (bps). =0: apply variable bit rate control; >0: apply constant bitrate control
//peak_bitrate = 6000000		// Highest bitrate allowed. Valid if applying constant bit rate control.
//vbv_buffer = 1835008		// VBV buffer size
//converge_speed = 100		// Converging speed of bit rate control process. 0(slowest) ~ 100(fastest)
//lambda = 100			// Stream quality factor. Smaller: better individual frame quality; Larger: smoother stream 
//Q = 0				// Initial quantizer, will be devided by 4, for exmaple, 7 represents 1.75
//IQ = 2				// Fixed quantize scale for I frame. Valid if target_bitrate=0 and Q=0.
//PQ = 2				// Fixed quantize scale for P frame. Valid if target_bitrate=0 and Q=0.
//BQ = 2				// Fixed quantize scale for B frame. Valid if target_bitrate=0 and Q=0.
